Device Name [AT86RF401]
flashSize   =  2048
eepromSize  =  128
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  145
signature2 =  129
pagesize   =  0
------------------------------

Device Name [AT89S51]
flashSize   =  4096
eepromSize  =  0
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  81
signature2 =  6
pagesize   =  1
------------------------------

Device Name [AT89S52]
flashSize   =  8192
eepromSize  =  0
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  82
signature2 =  6
pagesize   =  1
------------------------------

Device Name [AT90CAN128]
flashSize   =  131072
eepromSize  =  4096
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  151
signature2 =  129
pagesize   =  256
------------------------------

Device Name [AT90CAN32]
flashSize   =  32768
eepromSize  =  1024
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  149
signature2 =  129
pagesize   =  256
------------------------------

Device Name [AT90CAN64]
flashSize   =  65536
eepromSize  =  2048
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  150
signature2 =  129
pagesize   =  256
------------------------------

Device Name [AT90PWM2]
flashSize   =  8192
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  147
signature2 =  129
pagesize   =  64
------------------------------

Device Name [AT90PWM216]
flashSize   =  16384
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  148
signature2 =  131
pagesize   =  128
------------------------------

Device Name [AT90PWM2B]
flashSize   =  8192
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  147
signature2 =  131
pagesize   =  64
------------------------------

Device Name [AT90PWM3]
flashSize   =  8192
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  147
signature2 =  129
pagesize   =  64
------------------------------

Device Name [AT90PWM316]
flashSize   =  16384
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  148
signature2 =  131
pagesize   =  128
------------------------------

Device Name [AT90PWM3B]
flashSize   =  8192
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  147
signature2 =  131
pagesize   =  64
------------------------------

Device Name [AT90S1200]
flashSize   =  1024
eepromSize  =  64
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  144
signature2 =  1
pagesize   =  0
------------------------------

Device Name [AT90S2313]
flashSize   =  2048
eepromSize  =  128
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  145
signature2 =  1
pagesize   =  0
------------------------------

Device Name [AT90S2323]
flashSize   =  2048
eepromSize  =  128
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  145
signature2 =  2
pagesize   =  0
------------------------------

Device Name [AT90S2343]
flashSize   =  2048
eepromSize  =  128
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  145
signature2 =  3
pagesize   =  0
------------------------------

Device Name [AT90S4414]
flashSize   =  4096
eepromSize  =  256
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  146
signature2 =  1
pagesize   =  0
------------------------------

Device Name [AT90S4433]
flashSize   =  4096
eepromSize  =  256
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  146
signature2 =  3
pagesize   =  0
------------------------------

Device Name [AT90S4434]
flashSize   =  4096
eepromSize  =  256
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  147
signature2 =  3
pagesize   =  0
------------------------------

Device Name [AT90S8515]
flashSize   =  8192
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  147
signature2 =  1
pagesize   =  0
------------------------------

Device Name [AT90S8515comp]
flashSize   =  8192
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  147
signature2 =  1
pagesize   =  64
------------------------------

Device Name [AT90S8535]
flashSize   =  8192
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  147
signature2 =  3
pagesize   =  0
------------------------------

Device Name [AT90S8535comp]
flashSize   =  8192
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  147
signature2 =  3
pagesize   =  64
------------------------------

Device Name [AT90USB1286]
flashSize   =  131072
eepromSize  =  4096
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  151
signature2 =  130
pagesize   =  256
------------------------------

Device Name [AT90USB1287]
flashSize   =  131072
eepromSize  =  4096
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  151
signature2 =  130
pagesize   =  256
------------------------------

Device Name [AT90USB162]
flashSize   =  16384
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  148
signature2 =  130
pagesize   =  128
------------------------------

Device Name [AT90USB646]
flashSize   =  65536
eepromSize  =  2048
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  150
signature2 =  130
pagesize   =  256
------------------------------

Device Name [AT90USB647]
flashSize   =  65536
eepromSize  =  2048
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  150
signature2 =  130
pagesize   =  256
------------------------------

Device Name [AT90USB82]
flashSize   =  8192
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  147
signature2 =  130
pagesize   =  128
------------------------------

Device Name [ATmega103]
flashSize   =  131072
eepromSize  =  4096
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  151
signature2 =  1
pagesize   =  256
------------------------------

Device Name [ATmega103comp]
flashSize   =  131072
eepromSize  =  4096
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  151
signature2 =  1
pagesize   =  0
------------------------------

Device Name [ATmega128]
flashSize   =  131072
eepromSize  =  4096
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  151
signature2 =  2
pagesize   =  256
------------------------------

Device Name [ATmega1280]
flashSize   =  131072
eepromSize  =  4096
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  151
signature2 =  3
pagesize   =  256
------------------------------

Device Name [ATmega1281]
flashSize   =  131072
eepromSize  =  4096
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  151
signature2 =  4
pagesize   =  256
------------------------------

Device Name [ATmega16]
flashSize   =  16384
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  148
signature2 =  3
pagesize   =  128
------------------------------

Device Name [ATmega161]
flashSize   =  16384
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  148
signature2 =  1
pagesize   =  128
------------------------------

Device Name [ATmega161comp]
flashSize   =  16384
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  148
signature2 =  1
pagesize   =  128
------------------------------

Device Name [ATmega162]
flashSize   =  16384
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  148
signature2 =  4
pagesize   =  128
------------------------------

Device Name [ATmega163]
flashSize   =  16384
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  148
signature2 =  2
pagesize   =  128
------------------------------

Device Name [ATmega164P]
flashSize   =  16384
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  148
signature2 =  10
pagesize   =  256
------------------------------

Device Name [ATmega165]
flashSize   =  16384
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  148
signature2 =  7
pagesize   =  128
------------------------------

Device Name [ATmega165P]
flashSize   =  16384
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  148
signature2 =  7
pagesize   =  128
------------------------------

Device Name [ATmega168]
flashSize   =  16384
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  148
signature2 =  6
pagesize   =  128
------------------------------

Device Name [ATmega168P]
flashSize   =  16384
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  148
signature2 =  11
pagesize   =  128
------------------------------

Device Name [ATmega169]
flashSize   =  16384
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  148
signature2 =  5
pagesize   =  128
------------------------------

Device Name [ATmega169P]
flashSize   =  16384
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  148
signature2 =  5
pagesize   =  128
------------------------------

Device Name [ATmega16HVA]
flashSize   =  16384
eepromSize  =  256
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  148
signature2 =  12
pagesize   =  128
------------------------------

Device Name [ATmega2560]
flashSize   =  262144
eepromSize  =  4096
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  152
signature2 =  1
pagesize   =  256
------------------------------

Device Name [ATmega2561]
flashSize   =  262144
eepromSize  =  4096
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  152
signature2 =  2
pagesize   =  256
------------------------------

Device Name [ATmega32]
flashSize   =  32768
eepromSize  =  1024
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  149
signature2 =  2
pagesize   =  128
------------------------------

Device Name [ATmega323]
flashSize   =  32768
eepromSize  =  1024
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  149
signature2 =  1
pagesize   =  128
------------------------------

Device Name [ATmega324P]
flashSize   =  32768
eepromSize  =  1024
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  149
signature2 =  8
pagesize   =  128
------------------------------

Device Name [ATmega325]
flashSize   =  32768
eepromSize  =  1024
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  149
signature2 =  5
pagesize   =  128
------------------------------

Device Name [ATmega3250]
flashSize   =  32768
eepromSize  =  1024
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  149
signature2 =  6
pagesize   =  128
------------------------------

Device Name [ATmega3250P]
flashSize   =  32768
eepromSize  =  1024
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  149
signature2 =  110
pagesize   =  128
------------------------------

Device Name [ATmega325P]
flashSize   =  32768
eepromSize  =  1024
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  149
signature2 =  93
pagesize   =  128
------------------------------

Device Name [ATmega328P]
flashSize   =  32768
eepromSize  =  1024
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  149
signature2 =  15
pagesize   =  128
------------------------------

Device Name [ATmega329]
flashSize   =  32768
eepromSize  =  1024
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  149
signature2 =  3
pagesize   =  128
------------------------------

Device Name [ATmega3290]
flashSize   =  32768
eepromSize  =  1024
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  149
signature2 =  4
pagesize   =  128
------------------------------

Device Name [ATmega3290P]
flashSize   =  32768
eepromSize  =  1024
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  149
signature2 =  4
pagesize   =  128
------------------------------

Device Name [ATmega329P]
flashSize   =  32768
eepromSize  =  1024
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  149
signature2 =  3
pagesize   =  128
------------------------------

Device Name [ATmega406]
flashSize   =  40960
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  149
signature2 =  7
pagesize   =  128
------------------------------

Device Name [ATmega48]
flashSize   =  4096
eepromSize  =  256
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  146
signature2 =  5
pagesize   =  64
------------------------------

Device Name [ATmega48P]
flashSize   =  4096
eepromSize  =  256
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  146
signature2 =  10
pagesize   =  64
------------------------------

Device Name [ATmega64]
flashSize   =  65536
eepromSize  =  2048
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  150
signature2 =  2
pagesize   =  256
------------------------------

Device Name [ATmega640]
flashSize   =  65536
eepromSize  =  4096
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  150
signature2 =  8
pagesize   =  256
------------------------------

Device Name [ATmega644]
flashSize   =  65536
eepromSize  =  2048
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  150
signature2 =  9
pagesize   =  256
------------------------------

Device Name [ATmega644P]
flashSize   =  65536
eepromSize  =  2048
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  150
signature2 =  10
pagesize   =  256
------------------------------

Device Name [ATmega645]
flashSize   =  65536
eepromSize  =  2048
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  150
signature2 =  5
pagesize   =  256
------------------------------

Device Name [ATmega6450]
flashSize   =  65536
eepromSize  =  2048
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  150
signature2 =  6
pagesize   =  256
------------------------------

Device Name [ATmega649]
flashSize   =  65536
eepromSize  =  2048
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  150
signature2 =  3
pagesize   =  256
------------------------------

Device Name [ATmega6490]
flashSize   =  65536
eepromSize  =  2048
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  150
signature2 =  4
pagesize   =  256
------------------------------

Device Name [ATmega8]
flashSize   =  8192
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  147
signature2 =  7
pagesize   =  64
------------------------------

Device Name [ATmega8515]
flashSize   =  8192
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  147
signature2 =  6
pagesize   =  64
------------------------------

Device Name [ATmega8535]
flashSize   =  8192
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  147
signature2 =  8
pagesize   =  64
------------------------------

Device Name [ATmega88]
flashSize   =  8192
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  147
signature2 =  10
pagesize   =  64
------------------------------

Device Name [ATmega88P]
flashSize   =  8192
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  147
signature2 =  15
pagesize   =  64
------------------------------

Device Name [ATtiny11]
flashSize   =  1024
eepromSize  =  0
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  144
signature2 =  4
pagesize   =  0
------------------------------

Device Name [ATtiny12]
flashSize   =  1024
eepromSize  =  64
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  144
signature2 =  5
pagesize   =  0
------------------------------

Device Name [ATtiny13]
flashSize   =  1024
eepromSize  =  64
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  144
signature2 =  7
pagesize   =  32
------------------------------

Device Name [ATtiny15]
flashSize   =  1024
eepromSize  =  64
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  144
signature2 =  6
pagesize   =  0
------------------------------

Device Name [ATtiny22]
flashSize   =  2048
eepromSize  =  128
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  145
signature2 =  6
pagesize   =  0
------------------------------

Device Name [ATtiny2313]
flashSize   =  2048
eepromSize  =  128
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  145
signature2 =  10
pagesize   =  32
------------------------------

Device Name [ATtiny24]
flashSize   =  2048
eepromSize  =  128
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  145
signature2 =  11
pagesize   =  32
------------------------------

Device Name [ATtiny25]
flashSize   =  2048
eepromSize  =  128
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  145
signature2 =  8
pagesize   =  32
------------------------------

Device Name [ATtiny26]
flashSize   =  2048
eepromSize  =  128
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  145
signature2 =  9
pagesize   =  32
------------------------------

Device Name [ATtiny261]
flashSize   =  2048
eepromSize  =  128
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  145
signature2 =  12
pagesize   =  32
------------------------------

Device Name [ATtiny28]
flashSize   =  2048
eepromSize  =  0
hasFuseBits =  1
hasExtendedFuseBits =  0
signature0 =  30
signature1 =  145
signature2 =  7
pagesize   =  0
------------------------------

Device Name [ATtiny43U]
flashSize   =  4096
eepromSize  =  64
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  146
signature2 =  12
pagesize   =  32
------------------------------

Device Name [ATtiny44]
flashSize   =  4096
eepromSize  =  256
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  146
signature2 =  7
pagesize   =  64
------------------------------

Device Name [ATtiny45]
flashSize   =  4096
eepromSize  =  256
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  146
signature2 =  6
pagesize   =  64
------------------------------

Device Name [ATtiny461]
flashSize   =  4096
eepromSize  =  256
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  146
signature2 =  8
pagesize   =  64
------------------------------

Device Name [ATtiny48]
flashSize   =  4096
eepromSize  =  64
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  146
signature2 =  9
pagesize   =  64
------------------------------

Device Name [ATtiny84]
flashSize   =  8192
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  147
signature2 =  12
pagesize   =  64
------------------------------

Device Name [ATtiny85]
flashSize   =  8192
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  147
signature2 =  11
pagesize   =  64
------------------------------

Device Name [ATtiny861]
flashSize   =  8192
eepromSize  =  512
hasFuseBits =  1
hasExtendedFuseBits =  1
signature0 =  30
signature1 =  147
signature2 =  13
pagesize   =  64
------------------------------

